|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | ZP-35/37D Automatic Rotary Tablet Press Machine | | | | Share to： |  | | **ZP-35/37D Automatic Rotary Tablet Press Machine**   |  |  | | --- | --- | | Model： | ZP-35/37D | | Name： | Automatic Rotary Tablet Press Machine | |  |  | |  |  | |  |  | |
|  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Detail**  **APPLICATION**  The machine is a double pressing automatically revolving piece-pressing machine which could make grain be  pressed to be round pieces, be carved characters, special shapes and double color piece prescription. It is mainly  used in manufacturing piece prescription for pharmaceutical industry enterprises like chemical, food, electronics.  **FEATURE**  1. The inner machine surface already be special treated, which could keep surface luster and prevent from being  polluted crossly.  2. Equipped with over-load protection apparatus. When pressure overloads, the machine stop automatically.  3. Power suction unit is attached to take the residual power during operation so that the blockage powder can be  collected and be reused.  **TECHNICAL PARAMETER**   |  |  |  | | --- | --- | --- | | Model | ZP-35D | ZP-37D | | Dies | 35 | 37 | | Max. Pressure (KN) | 80 | 80 | | Max. Tablet Dia. (mm) | 13 | 13 | | Max. Filling Depth (mm) | 15 | 15 | | Max. Thickness (mm) | 6 | 6 | | Production Capacity (pcs/h) | 150000 | 160000 | | Motor (KW) | 4 | 4 | | Overall Dimensions (mm) | 980×1240×1690 | 980×1240×1690 | | Net Weight (KG) | 1700 | 1700 | |