**SJ-2L Automatic Suppository Packing Machine**

****

|  |  |  |  |
| --- | --- | --- | --- |
| Product Name | Suppository Line | Model | SJ-2L |
| Output | 3000-3600 pcs/h | Dosage | 0.5—5ml |
| Dosage allowed | ＜±2% | Packaging Film | PVC PVC\PE  Thickness 0.15mm |
| Storage of the liquid barrel | 20L | Atmospheric pressure | ≥0.6Mpa |
| Consume the tolerance | 1.0m3 | Water quantity | 50kg (Circling) |
| Voltage | 380V | Total power | 3KW |
| Shapes | Different | Weight | 500kg |
| Dimension | 2000×1500×1600 | Each distance of suppository | 17.4mm |

**Electronic Part List**

|  |  |  |
| --- | --- | --- |
| No. | Name | Brand |
| 1 | PLC | Siemens |
|  | Communication module | Siemens |
|  | Temperature Module | Siemens |
| 2 | Touch Screen | Siemens |
| 3 | Frequency Convetor | Schneider |
| 4 | Breaker | Schneider |
| 5 | Temperature Control | Yudian |
| 6 | Solenoid Valve | AirTAC |
| 7 | Sensor | Schneider |
| 8 | Alarming Buzzer | China |

Price 72000$ CIF